Firmware Updating Instructions S8300 – Option 1

1. Insert USB Drive into USB Port on the Rear of the S8300.

2. Go to Menu/ Software Upgrade/ Manual Update, select “USB” from options and press “OK”.

3. Read on screen notification and enter Password (Default Password is “0000”).

4. Unit will then begin the software update, when complete it will resume normal TV viewing.

WARNING! DO NOT REMOVE POWER TO THE UNIT WHEN UPDATING

Firmware Updating Instructions S8200 – Option 2

1. Power off your S8300 at the wall.

2. Insert USB Drive into the USB Port on the Rear of the unit.

3. Hold the “DOWN” Button down on the Front Panel of the S8300; reconnect the power while still holding it down.

4. After few seconds “UPG” will come up on the front display, allowing you to release “DOWN”.

6. Unit will then begin the software update, when complete it will resume normal TV viewing.

WARNING! DO NOT REMOVE POWER TO THE UNIT WHEN UPDATING